[stereoscopic_video_info_descriptor.UpsamplingFactor]
Bits = 4
0 = Forbidden
1 = Unspecified
2 = Same as coded resolution of base view
3 = 3/4 coded resolution of base view
4 = 2/3 coded resolution of base view
5 = 1/2 coded resolution of base view
