#
# TSDuck - The MPEG Transport Stream Toolkit
# Copyright (c) 2005-2023, Thierry Lelegard
# BSD-2-Clause license, see LICENSE.txt file or https://tsduck.io/license
#
# Configuration file containing names for Internet protocols.
#

[IPProtocol]
# Protocol codes over IP (TCP, UDP, etc.)
# Format is "acronym: description"
# See: https://en.wikipedia.org/wiki/List_of_IP_protocol_numbers
Bits = 8
0x00 = HOPOPT: IPv6 Hop-by-Hop Option
0x01 = ICMP: Internet Control Message Protocol
0x02 = IGMP: Internet Group Management Protocol
0x03 = GGP: Gateway-to-Gateway Protocol
0x04 = IP-in-IP: IP in IP encapsulation
0x05 = ST: Internet Stream Protocol
0x06 = TCP: Transmission Control Protocol
0x07 = CBT: Core-based trees
0x08 = EGP: Exterior Gateway Protocol
0x09 = IGP: Interior Gateway Protocol
0x0A = BBN-RCC-MON: BBN RCC Monitoring
0x0B = NVP-II: Network Voice Protocol
0x0C = PUP: Xerox PUP
0x0D = ARGUS: ARGUS
0x0E = EMCON: EMCON
0x0F = XNET: Cross Net Debugger
0x10 = CHAOS: Chaos
0x11 = UDP: User Datagram Protocol
0x12 = MUX: Multiplexing
0x13 = DCN-MEAS: DCN Measurement Subsystems
0x14 = HMP: Host Monitoring Protocol
0x15 = PRM: Packet Radio Measurement
0x16 = XNS-IDP: XEROX NS IDP
0x17 = TRUNK-1: Trunk-1
0x18 = TRUNK-2: Trunk-2
0x19 = LEAF-1: Leaf-1
0x1A = LEAF-2: Leaf-2
0x1B = RDP: Reliable Data Protocol
0x1C = IRTP: Internet Reliable Transaction Protocol
0x1D = ISO-TP4: ISO Transport Protocol Class 4
0x1E = NETBLT: Bulk Data Transfer Protocol
0x1F = MFE-NSP: MFE Network Services Protocol
0x20 = MERIT-INP: MERIT Internodal Protocol
0x21 = DCCP: Datagram Congestion Control Protocol
0x22 = 3PC: Third Party Connect Protocol
0x23 = IDPR: Inter-Domain Policy Routing Protocol
0x24 = XTP: Xpress Transport Protocol
0x25 = DDP: Datagram Delivery Protocol
0x26 = IDPR-CMTP: IDPR Control Message Transport Protocol
0x27 = TP++: TP++ Transport Protocol
0x28 = IL: IL Transport Protocol
0x29 = IPv6: IPv6 Encapsulation
0x2A = SDRP: Source Demand Routing Protocol
0x2B = IPv6-Route: Routing Header for IPv6
0x2C = IPv6-Frag: Fragment Header for IPv6
0x2D = IDRP: Inter-Domain Routing Protocol
0x2E = RSVP: Resource Reservation Protocol
0x2F = GRE: Generic Routing Encapsulation
0x30 = DSR: Dynamic Source Routing Protocol
0x31 = BNA: Burroughs Network Architecture
0x32 = ESP: Encapsulating Security Payload
0x33 = AH: Authentication Header
0x34 = I-NLSP: Integrated Net Layer Security Protocol TUBA
0x35 = SwIPe: SwIPe
0x36 = NARP: NBMA Address Resolution Protocol
0x37 = MOBILE: IP Mobility (Min Encap)
0x38 = TLSP: Transport Layer Security Protocol
0x39 = SKIP: Simple Key-Management for Internet Protocol
0x3A = IPv6-ICMP: ICMP for IPv6
0x3B = IPv6-NoNxt: No Next Header for IPv6
0x3C = IPv6-Opts: Destination Options for IPv6
0x3E = CFTP: CFTP
0x40 = SAT-EXPAK: SATNET and Backroom EXPAK
0x41 = KRYPTOLAN: Kryptolan
0x42 = RVD: MIT Remote Virtual Disk Protocol
0x43 = IPPC: Internet Pluribus Packet Core
0x45 = SAT-MON: SATNET Monitoring
0x46 = VISA: VISA Protocol
0x47 = IPCU: Internet Packet Core Utility
0x48 = CPNX: Computer Protocol Network Executive
0x49 = CPHB: Computer Protocol Heart Beat
0x4A = WSN: Wang Span Network
0x4B = PVP: Packet Video Protocol
0x4C = BR-SAT-MON: Backroom SATNET Monitoring
0x4D = SUN-ND: SUN ND PROTOCOL-Temporary
0x4E = WB-MON: WIDEBAND Monitoring
0x4F = WB-EXPAK: WIDEBAND EXPAK
0x50 = ISO-IP: International Organization for Standardization Internet Protocol
0x51 = VMTP: Versatile Message Transaction Protocol
0x52 = SECURE-VMTP: Secure Versatile Message Transaction Protocol
0x53 = VINES: VINES
0x54 = IPTM: Internet Protocol Traffic Manager
0x55 = NSFNET-IGP: NSFNET-IGP
0x56 = DGP: Dissimilar Gateway Protocol
0x57 = TCF: TCF
0x58 = EIGRP: EIGRP Informational
0x59 = OSPF: Open Shortest Path First
0x5A = Sprite-RPC: Sprite RPC Protocol
0x5B = LARP: Locus Address Resolution Protocol
0x5C = MTP: Multicast Transport Protocol
0x5D = AX.25: AX.25
0x5E = OS: KA9Q NOS compatible IP over IP tunneling
0x5F = MICP: Mobile Internetworking Control Protocol
0x60 = SCC-SP: Semaphore Communications Sec. Pro
0x61 = ETHERIP: Ethernet-within-IP Encapsulation
0x62 = ENCAP: Encapsulation Header
0x64 = GMTP: GMTP
0x65 = IFMP: Ipsilon Flow Management Protocol
0x66 = PNNI: PNNI over IP
0x67 = PIM: Protocol Independent Multicast
0x68 = ARIS: IBM's ARIS (Aggregate Route IP Switching) Protocol
0x69 = SCPS: Space Communications Protocol Standards
0x6A = QNX: QNX
0x6B = A/N: Active Networks
0x6C = IPComp: IP Payload Compression Protocol
0x6D = SNP: Sitara Networks Protocol
0x6E = Compaq-Peer: Compaq Peer Protocol
0x6F = IPX-in-IP: IPX in IP
0x70 = VRRP: Virtual Router Redundancy Protocol
0x71 = PGM: PGM Reliable Transport Protocol
0x73 = L2TP: Layer Two Tunneling Protocol Version 3
0x74 = DDX: D-II Data Exchange
0x75 = IATP: Interactive Agent Transfer Protocol
0x76 = STP: Schedule Transfer Protocol
0x77 = SRP: SpectraLink Radio Protocol
0x78 = UTI: Universal Transport Interface Protocol
0x79 = SMP: Simple Message Protocol
0x7A = SM: Simple Multicast Protocol
0x7B = PTP: Performance Transparency Protocol
0x7C = IS-IS-over-IPv4: Intermediate System to Intermediate System (IS-IS) Protocol
0x7D = FIRE: Flexible Intra-AS Routing Environment
0x7E = CRTP: Combat Radio Transport Protocol
0x7F = CRUDP: Combat Radio User Datagram
0x80 = SSCOPMCE: Service-Specific Connection-Oriented Protocol in a Multilink and Connectionless Environment
0x81 = IPLT: IPLT
0x82 = SPS: Secure Packet Shield
0x83 = PIPE: Private IP Encapsulation within IP
0x84 = SCTP: Stream Control Transmission Protocol
0x85 = FC: Fibre Channel
0x86 = RSVP-E2E-IGNORE: Reservation Protocol (RSVP) End-to-End Ignore
0x87 = Mobility-Header: Mobility Extension Header for IPv6
0x88 = UDPLite: Lightweight User Datagram Protocol
0x89 = MPLS-in-IP: Multiprotocol Label Switching Encapsulated in IP
0x8A = MANET: MANET Protocols
0x8B = HIP: Host Identity Protocol
0x8C = Shim6: Site Multihoming by IPv6 Intermediation
0x8D = WESP: Wrapped Encapsulating Security Payload
0x8E = ROHC: Robust Header Compression
0x8F = Ethernet: IPv6 Segment Routing
