[RNT.ContextIdType]
# In Resolution provider Notification Table
Bits = 8
0x00 = context_id is a bouquet_id
0x01 = context_id is an original_network_id
0x02 = context_id is a network_id
0x03-0x7F = DVB reserved
0x80-0xFF = User defined

[RNT.AuthorityPolicy]
# In Resolution provider Notification Table
Bits = 2
0 = CRID's are permanent
1 = CRID's are transient
2 = CRID's may be either transient or permanent
3 = Reserved
