[basic_local_event_descriptor.Mode]
# In ISDB basic_local_event_descriptor
Bits = 4
0 = Invalid
1 = NPT
2 = Relative time
3 = Relative time (STC reference descriptor is used together)
4 = JST time
5 = JST time (STC reference descriptor is used together)
6-15 = Reserved
