[SAT.satellite_table_id]
Bits = 6
0x00 = Satellite Position V2
0x01 = Cell Fragment
0x02 = Time Association
0x03 = Beamhopping Time Plan

[SAT.west_east_indicator]
Bits = 1
0 = west
1 = east

[SAT.UTC_mode]
Bits = 4
0 = without leap second signalling
1 = with leap second signalling

[SAT.time_plan_mode]
Bits = 2
0 = one transmission each cycle
1 = multiple transmission each cycle
2 = only grid size is siganlled, not illuminance
