====================================================
TSDuck - List of features to be implemented or fixed
====================================================

* Issue #324: Fix tsswitch --delayed-switch --receive-timeout.

* Implement missing PSI/SI tables and descriptors (list below).

  ISO/IEC 13818-1 / H.222 (MPEG system layer)
  - With embedded data structures from ISO/IEC 14496-1 (MPEG-4 system):
    - 2.6.40   IOD_descriptor
  - With embedded data structures from ISO/IEC 14496-3 (MPEG-4 Audio):
    - 2.6.72   MPEG4_audio_extension_descriptor
  - With embedded data structures from ISO/IEC 23002-3 (MPEG-C auxiliairy video):
    - 2.6.74   auxiliary_video_stream_descriptor
  - With embedded data structures from ISO/IEC 23008-3 (High efficiency 3D audio):
    - 2.6.108  MPEGH_3D_audio_config_descriptor
    - 2.6.116  MPEGH_3D_audio_DRC_loudness_descriptor
    - 2.6.118  MPEGH_3D_audio_command_descriptor

  ETSI TS 102 323 (Carriage and signalling of TV-Anytime information)
  - 10.4.2  RCT (Related Content Table)

  ARIB STD-B10 (ISDB Service Information)
  - Part 2:
    - 6.2.46  carousel_compatible_composite_descriptor

  ARIB STD-B21 (ISDB Receiver for Digital Broadcasting)
  - 9.1.8.3   partial_transport_stream_time_descriptor
  - 9.1.8.3   partial_TS_time_descriptor
  - 12.2.1.1  SDTT (Software Download Trigger Table)
  - 12.2.1.1  download_content_descriptor

  ARIB STD-B16 (ISDB Standard Digital Receiver for Satellite - not available in English)
  - DCT (Download Control Table)
  - DLT (DownLoad Table)
